Insert Worksite Logo Here

EMERGENCY PROCEDURE FOR A GAS LEAK

Upon discovery of a gas leak:

**IMMEDIATE ACTIONS**

* **DO NOT** **turn on** any light/power switch or any electrical equipment

(*it might create an ignition source)*

* Activate the gas isolation/emergency stop.
* Follow site emergency/evacuation procedure.
* If safe to do so:
  + Check all gas outlets and close any that have been left open.
  + Identify source of gas leak.

**FOLLOWING ACTIONS**

* Do not allow any other person to enter the room.
* Open all doors and windows.
* Once the room is clear of the smell of gas have a competent person check the room before allowing re-entry.
* If the cause of the gas leak is not obvious contact a gas plumber.

If the smell of gas is still obvious after ventilating the room call the emergency services on 000.