|  |  |  |
| --- | --- | --- |
|  | **HOT WORK PERMIT FOR CONFINED SPACE**  |  |
| **Workplace:** | **Location:** | **Date:** |

**The precautions ticked below must be fully observed.**

(1) The area is clean and free of **all** readily combustible materials within 15 metres. ⬜

(2) **All** drains within 15 metres are covered with a wet fireproof blanket. ⬜

(3) Appropriate fire extinguishers are on site and near the source of ignition. ⬜

(4) A water hose is run to the job site, tested/left running. ⬜

(5) All sparks from work conducted more than 2 metres above ground, **must** be contained

completely by the use of a suitable enclosure that **shall be inspected** before

commencing work. ⬜

(6) Welding machine/gas cylinders are located (they **must not** be within 8 metres of

any drain). ⬜

(7) Welding machine must be earthed directly to the equipment that is being welded as

close to the welding point as practical. ⬜

(8) Power leads are not draped across pipelines or access ways. ⬜

(9) Electrical traces on pipes are isolated. ⬜

**Any special conditions?**

***I have read and fully understand the precautions of hot work in confined spaces as per AS 2865:2001 (safe work in a confined space) and HB 213:2003 (Guidelines for safe working in a confined space)***

**AUTHORISATION**

The hot work in or on the occupied confined space described above and on the associated Written Authority, is in my opinion, safe for the work to be carried out, provided that the precautions listed are adhered to.

Signature: Date: \_\_\_/\_\_\_/\_\_\_ Time: \_\_\_\_\_ am/pm

 Date: \_\_\_/\_\_\_/\_\_\_ Time: \_\_\_\_\_

 Date: \_\_\_/\_\_\_/\_\_\_ Time: \_\_\_\_\_

 Competent Person(s) entering or person in direct control